Performance

|  |  |  |
| --- | --- | --- |
| Acceleration 0 - 100 km/h | | 6.3 sec |
| Top Speed | | 180 km/h |
| Electric Range \* | | 400 km |
| Total Power | 220 kW (299 PS) | |
| Total Torque | 460 Nm | |
| Drive | AWD | |

Battery

|  |  |  |
| --- | --- | --- |
| Nominal Capacity | 82.0 kWh | |
| Battery Type | Lithium-ion | |
| Number of Cells | 288 | |
| Architecture | 400 V | |
| Warranty Period | No Data | |
| Warranty Mileage | No Data | |
| Useable Capacity | | 77.0 kWh |
| Cathode Material | | No Data |
| Pack Configuration | | 96s3p |
| Nominal Voltage | | No Data |
| Form Factor | | No Data |
| Name / Reference | | No Data |

Charging

Home / Destination

|  |  |  |
| --- | --- | --- |
| Charge Port | Type 2 | |
| Port Location | Right Side - Rear | |
| Charge Power | 11 kW AC | |
| Charge Time (0->400 km) | | 8h15m |
| Charge Speed | | 49 km/h |

Fast Charging

|  |  |  |
| --- | --- | --- |
| Fastcharge Port | CCS | |
| FC Port Location | Right Side - Rear | |
| Fastcharge Power (max) | 175 kW DC | |
| Fastcharge Power (10-80%) | 115 kW DC | |
| Fastcharge Time (40->320 km) | | 30 min |
| Fastcharge Speed | | 560 km/h |
| Autocharge Supported | | No |

Plug & Charge

|  |  |  |
| --- | --- | --- |
| Plug & Charge Supported | | Yes |
| Supported Protocol | ISO 15118-2 | |

Bidirectional Charging (V2X / BPT)

Vehicle-to-Load (V2L)

|  |  |  |
| --- | --- | --- |
| V2L Supported | No | |
| Max. Output Power | - | |
| Exterior Outlet(s) | | - |
| Interior Outlet(s) | | - |

Vehicle-to-Home (V2H)

|  |  |  |
| --- | --- | --- |
| V2H via AC Supported | | No |
| Max. Output Power | | - |
| V2H via DC Supported | Announced | |
| Max. Output Power | 10.0 kW DC | |

Vehicle-to-Grid (V2G)

|  |  |  |
| --- | --- | --- |
| V2G via AC Supported | | No |
| Max. Output Power | | - |
| V2G via DC Supported | Announced | |
| Max. Output Power | 10.0 kW DC | |

Energy Consumption

EVDB Real Range

|  |  |  |
| --- | --- | --- |
| Range \* | 400 km | |
| Vehicle Consumption \* | 193 Wh/km | |
| CO2 Emissions | | 0 g/km |
| Vehicle Fuel Equivalent \* | | 2.2 l/100km |

WLTP Ratings (TEL)

|  |  |
| --- | --- |
| Range | 509 km |
| Rated Consumption | 172 Wh/km |
| Vehicle Consumption | 151 Wh/km |
| CO2 Emissions | 0 g/km |
| Rated Fuel Equivalent | 1.9 l/100km |
| Vehicle Fuel Equivalent | 1.7 l/100km |

WLTP Ratings (TEH)

|  |  |
| --- | --- |
| Range | 490 km |
| Rated Consumption | 180 Wh/km |
| Vehicle Consumption | 157 Wh/km |
| CO2 Emissions | 0 g/km |
| Rated Fuel Equivalent | 2.0 l/100km |
| Vehicle Fuel Equivalent | 1.8 l/100km |

Safety (Euro NCAP)

|  |  |  |
| --- | --- | --- |
| Safety Rating |  | |
| Adult Occupant | 93% | |
| Child Occupant | 89% | |
| Rating Year | | 2021 |
| Vulnerable Road Users | | 76% |
| Safety Assist | | 85% |

For more details on the safety rating of this vehicle, visit [euroncap.com](https://www.euroncap.com/en/results/vw/id.4/42456)

Dimensions and Weight

|  |  |  |
| --- | --- | --- |
| Length | | 4584 mm |
| Width | | 1852 mm |
| Width with mirrors | | No Data |
| Height | | 1631 mm |
| Wheelbase | | 2771 mm |
| Weight Unladen (EU) | | 2239 kg |
| Gross Vehicle Weight (GVWR) | | 2750 kg |
| Max. Payload | | 586 kg |
| Cargo Volume | 543 L | |
| Cargo Volume Max | 1575 L | |
| Cargo Volume Frunk | 0 L | |
| Roof Load | 75 kg | |
| Tow Hitch Possible | Yes | |
| Towing Weight Unbraked | 750 kg | |
| Towing Weight Braked | 1200 kg | |
| Vertical Load Max | 75 kg | |

Miscellaneous

|  |  |
| --- | --- |
| Seats | 5 people |
| Isofix | Yes, 3 seats |
| Turning Circle | 11.6 m |
| Platform | VW MEB |
| EV Dedicated Platform | Yes |
| Car Body | SUV |
| Segment | JC - Medium |
| Roof Rails | Yes |
| Heat pump (HP) | Yes |
| HP Standard Equipment | No, optional |