Performance

|  |  |
| --- | --- |
| Acceleration 0 - 100 km/h | 6.3 sec |
| Top Speed | 180 km/h |
| Electric Range \* | 400 km |
| Total Power | 220 kW (299 PS) |
| Total Torque | 460 Nm |
| Drive | AWD |

Battery

|  |  |
| --- | --- |
| Nominal Capacity | 82.0 kWh |
| Battery Type | Lithium-ion |
| Number of Cells | 288 |
| Architecture | 400 V |
| Warranty Period | No Data |
| Warranty Mileage | No Data |
| Useable Capacity | 77.0 kWh |
| Cathode Material | No Data |
| Pack Configuration | 96s3p |
| Nominal Voltage | No Data |
| Form Factor | No Data |
| Name / Reference | No Data |

Charging

Home / Destination

|  |  |
| --- | --- |
| Charge Port | Type 2 |
| Port Location | Right Side - Rear |
| Charge Power | 11 kW AC |
| Charge Time (0->400 km) | 8h15m |
| Charge Speed | 49 km/h |

Fast Charging

|  |  |
| --- | --- |
| Fastcharge Port | CCS |
| FC Port Location | Right Side - Rear |
| Fastcharge Power (max) | 175 kW DC |
| Fastcharge Power (10-80%) | 115 kW DC |
| Fastcharge Time (40->320 km) | 30 min |
| Fastcharge Speed | 560 km/h |
| Autocharge Supported | No |

Plug & Charge

|  |  |
| --- | --- |
| Plug & Charge Supported | Yes |
| Supported Protocol | ISO 15118-2 |

Bidirectional Charging (V2X / BPT)

Vehicle-to-Load (V2L)

|  |  |
| --- | --- |
| V2L Supported | No |
| Max. Output Power | - |
| Exterior Outlet(s) | - |
| Interior Outlet(s) | - |

Vehicle-to-Home (V2H)

|  |  |
| --- | --- |
| V2H via AC Supported | No |
| Max. Output Power | - |
| V2H via DC Supported | Announced |
| Max. Output Power | 10.0 kW DC |

Vehicle-to-Grid (V2G)

|  |  |
| --- | --- |
| V2G via AC Supported | No |
| Max. Output Power | - |
| V2G via DC Supported | Announced |
| Max. Output Power | 10.0 kW DC |

Energy Consumption

EVDB Real Range

|  |  |
| --- | --- |
| Range \* | 400 km |
| Vehicle Consumption \* | 193 Wh/km |
| CO2 Emissions | 0 g/km |
| Vehicle Fuel Equivalent \*  | 2.2 l/100km |

WLTP Ratings (TEL)

|  |  |
| --- | --- |
| Range | 509 km |
| Rated Consumption | 172 Wh/km |
| Vehicle Consumption | 151 Wh/km |
| CO2 Emissions | 0 g/km |
| Rated Fuel Equivalent | 1.9 l/100km |
| Vehicle Fuel Equivalent | 1.7 l/100km |

WLTP Ratings (TEH)

|  |  |
| --- | --- |
| Range | 490 km |
| Rated Consumption | 180 Wh/km |
| Vehicle Consumption | 157 Wh/km |
| CO2 Emissions | 0 g/km |
| Rated Fuel Equivalent | 2.0 l/100km |
| Vehicle Fuel Equivalent | 1.8 l/100km |

Safety (Euro NCAP)

|  |  |
| --- | --- |
| Safety Rating |  |
| Adult Occupant | 93% |
| Child Occupant | 89% |
| Rating Year | 2021 |
| Vulnerable Road Users | 76% |
| Safety Assist | 85% |

For more details on the safety rating of this vehicle, visit [euroncap.com](https://www.euroncap.com/en/results/vw/id.4/42456)

Dimensions and Weight

|  |  |
| --- | --- |
| Length | 4584 mm |
| Width | 1852 mm |
| Width with mirrors | No Data |
| Height | 1631 mm |
| Wheelbase | 2771 mm |
| Weight Unladen (EU) | 2239 kg |
| Gross Vehicle Weight (GVWR) | 2750 kg |
| Max. Payload | 586 kg |
| Cargo Volume | 543 L |
| Cargo Volume Max | 1575 L |
| Cargo Volume Frunk | 0 L |
| Roof Load | 75 kg |
| Tow Hitch Possible | Yes |
| Towing Weight Unbraked | 750 kg |
| Towing Weight Braked | 1200 kg |
| Vertical Load Max | 75 kg |

Miscellaneous

|  |  |
| --- | --- |
| Seats  | 5 people |
| Isofix | Yes, 3 seats |
| Turning Circle | 11.6 m |
| Platform | VW MEB |
| EV Dedicated Platform | Yes |
| Car Body | SUV |
| Segment | JC - Medium |
| Roof Rails | Yes |
| Heat pump (HP) | Yes |
| HP Standard Equipment | No, optional |